**Code Quality Report**

GEAR

**(Process Control Metrics)**

**Reader Name:** DM260-3D3420

**Device Type:** DM260

**Serial Number:** 1A1615XN007410

**Software Version:** 5.7.0\_sr2

**Trigger Index:** 4849

Result (raw):

**Overall Result: PASS Specification:** AIM-DPM **Symbology:** Data Matrix

**Symbol Size:** 20 columns / 20 rows

**Pixel Per Cell:** 3.680

Image:

****

Detailed Results:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Quality Parameter** | **Result (Raw)** | **Grade** | **Min** | **Max** | **Avg** | **Dev** |
| Overall Grade |  | A |  |  |  |  |
| Cell Contrast | 0.578 | A | 0.449 | 0.817 | 0.696 | 0.083 |
| Axial Non Uniformity | 0.056 | A | 0.001 | 0.199 | 0.064 | 0.026 |
| Print Growth | -0.039 |  | -0.039 | 0.156 | 0.090 | 0.036 |
| UEC | 1.000 | A | 0.000 | 1.000 | 0.676 | 0.259 |
| Cell Modulation |  | A |  |  |  |  |
| Fixed Pattern Damage |  | A |  |  |  |  |
| Grid Non Uniformity | 0.172 | A | 0.009 | 0.707 | 0.348 | 0.134 |